Reset Voicemail Through OXO Phone

* Hit the left arrow key to toggle to the “Menu” tab
* Press the key labeled “Operator”
* It will prompt you for a password
* Then use the number pad and keyboard to type the password “Help1954”
* Press OK
* Press the key labeled “Subscr”
* Use your dial pad to enter the extension number needing a password reset
* Select the key labeled “PwdRes”
* Select “OK” to confirm
* Hit the red hangup key.
* Your password should now be reset to 852000

--- If the password “Help1954” or “852000” does not work I will have to come out on-site or access remotely to reset the voicemail box.